# Introduction

„Cookery-book“

for your first programming example for the XC164CS Step AA Starterkit-Board in 9 Steps:

your program:
| *** Recipes ***
I.) | ## XC16x Board Power Supply the correct Jumper Setting (please refer to the XC16Board Hardware Manual) serial cable to the notebook
II.) | ## DAvE – program generator you need a installed version of the DAvE 2 CD ROM you need the DAvE Update for XC16x microcontrollers (XC164CS_v21.DIP)
III.) | using DAvE microcontroller initialization for your programming example
(either:) IV.) | using the KEIL Development Tools (C/EC++ Compiler) Programming of your application (e10k) with KEIL tool chain (µVision2)
(or:) V.) | using the TASKING Development Tools (C/C++/EC++ Compiler) Programming of your application (e10t) with TASKING (Altium) tool chain (EDE)
VI.) | #### MEMTOOL Installation You need this Tool for the programming of the OnChipFlash in the XC164CS.
VII.) | ### using MEMTOOL for KEIL: programming of e10k.h86 into the OnChipFlash memory for TASKING: programming of e10t.hex into the OnChipFlash memory
VIII.) | #### Terminal – Settings using a terminal program (settings)
IX.) | using a Terminalprogram Screenshots of your running application