II.) DAvE – Update Installation for XC16x microcontrollers:

1.) Copy the files “XC161CJ_v21.DIP “ and “XC164CS_v21.DIP“ under the installation path of DAvE ( C:\Programme\DAvE ).
2.) Start DAvE
3.) View Setup Wizard Default: · Installation # Forward> Select: · I want to install products from the DAvE’s web site ## Forward> Select: C:\Programme\DAvE ## Forward> Select: Available Products a XC161CJ a XC164CS ## Forward> ## Install End
DAvE is now ready to generate code for XC161CJ and XC164CS microcontrollers.